Author: Malori Carr

HES Technical Training Documentation: Fixtures

SolaFrame 750	SolaSpot 1000	SolaHyBeam 1000	SolaWash 19	QUAD
SolaFrame 1000	SolaSpot 2000	SolaHyBeam 2000	SolaWash 2000
SolaFrame 2000	SolaSpot 3000
SolaFrame 3000
SolaFrame Theatre

Website– High End Home	KMS– Knowledge Management System	Legacy Products	HES Support Contacts	Automated Lighting Pricelist

SolaWash 2000

SolaWash 2000

Accessing the Electronics

Remove 4X Philips head screws on each top cover
Disconnect Ground Wire underneath covers
Remove 5X Philips head screws on the front and rear panel covers

PCB Junction Base

SolaWash 2000

Front Panel Components

LED Driver

LED Power Supply 52VDC Output

PCB 3U: LED Control

PCB 1U: Display

SolaWash 2000

Rear Panel Components

LED Distribution

LED Power Supply 52VDC Output

Motor Power Supply 28VDC Output

Mains Fuse

Display Battery

XLR PCB 3 & 5 Pin

Powercon Connector

DC Wiring:
Blue is -
Red is +

SolaWash 2000

Removing the Motor Power Supply

Lay the fixture carefully on its side
Remove 4X rubber feet using a 3mm HEX tool
Remove 2X Philips head screws

SolaWash 2000

Removing the Motor Power Supply

Remove output power connectors
Remove2X Philips head screws
Remove input power connections
Remove 2X Philips screws
Remove 3X mounting screws and install onto new Power Supply
Remove 2X Philips head screws

Add heat sink compound to the new Power Supply before installing onto a mounting plate

SolaWash 2000

Removing LED Power Supply

Remove 2X front mounting screws using magnetized Philips head
Remove 2X rear mounting screws

SolaWash 2000

Removing LED Power Supply

Disconnect power connector
Loosen 4X silver Philips screws and disconnect output wires from the terminal block

Remove the Power Supply mount by removing 2X Philips screws

Apply heat sink compound to the original mount and install on the new Power Supply

SolaWash 2000

Accessing the Yoke

Remove yoke arm cover screws, 2 on each side

Tilt Homing Sensor

Sensor Tilt Encoder

PCB 2U: Pan/Tilt

Sensor Pan Encoder

SolaWash 2000

Accessing the Pan Homing Sensor/Removing Yoke Covers

Remove yoke cover on Pan/Tilt PCB Side:
Remove 2X screws at the top
Remove 4X screws through access holes
Note the different screw types
Loosen 2X yoke cover screws on the front/rear of the yoke

SolaWash 2000

Accessing the Pan Homing Sensor/Removing Yoke Covers

Remove yoke cover on Tilt Belt side:
Remove 2X screws at the top
Remove 4X screws towards the bottom
Note the different screw types

Pan Homing Sensor

Loosen 2X cover screws on the front/rear of the fixture

SolaWash 2000

Head Components

Framing Module

Loosen 2X captive 1/4 screws, on each side

Frost Assembly
Top: Heavy, Bottom: Light

Pan Homing Sensor

Pan Homing Sensor

PCB 4U: Focus, Frost Zoom

Color Module

LED Intake Fans

PCB 5U: Color Mix, Color Wheels

LED Exhaust Fans

SolaWash 2000

Removing the Color Mix Module

Remove 2x module harness connectors
If thumb screws are used, feel free to remove completely as they are no longer used in production units

Remove 2X Philips head screws
Carefully pull out module

SolaWash 2000

Removing the Framing Module

Pull up on the focus & zoom assembly or tilt the fixture head downward to clear the path for the module to be removed
Unseat 2X module harness connects

Remove 2X Philips head screws
Carefully pull out module

SolaWash 2000

Removing the Front Head Cover

Remove 4X Philips Head screws, 2 on each side
Disconnect Safety Cable

SolaWash 2000

Replacing the LED Light Engine

Remove the Framing Module and Color Module, see earlier pages
Disconnect LED Harness on both side
Note the different sized connectors

SolaWash 2000

SolaWash 2000

Replacing the LED Light Engine

Remove 4X Philips head screws
Remove LED Heatsink by supporting heat sink and removing 4X Philips head screws
Carefully remove LED Heatsink
Mind the heatsink compound on the front of the heatsink

SolaWash 2000

SolaWash 2000

Replacing the LED Light Engine

Remove 4X Hex screws using 3mm Hex tool

Apply fresh heatsink compound to the new LED Light Engine before installing

SolaWash 2000

SolaWash 2000

PCB Identifiers

PCB Software ID	Controls
1U	Display
2U	Pan, Tilt
3U	LED Control
4U	Focus, Zoom, Frost 1
5U	CMY, CTO, Color Wheel
6U	Blade 4, Iris, Frost 2
7U	Blades 1-3, Framing Rotation

#